<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
</plain>
<libraries>
<library name="SPCoast">
<packages>
<package name="BOARD-DINRAIL-3.17INX10CM">
</package>
<package name="RJ45-NO-SHIELD">
<description>RJ45 Low Profile panel mount, no shield
For all RJ45 N and Z Series Models&lt;br&gt;
Source: www.tycoelectronics.com .. ENG_DS_1654001_1099_RJ_L_0507.pdf</description>
</package>
<package name="RJ24-INVERTED-PINS">
</package>
<package name="FIDUCIAL_1MM">
</package>
<package name="0603-LED">
<description>OSRAM CHIPLED</description>
</package>
<package name="0603-RES">
</package>
<package name="MAX4702EUE+">
</package>
<package name="SOT363">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BOARD1" library="SPCoast" package="BOARD-DINRAIL-3.17INX10CM" value=""/>
<element name="CON-AA" library="SPCoast" package="RJ45-NO-SHIELD" value="">
<attribute name="OPL" value="none"/>
<attribute name="AMP" value="520151-4"/>
</element>
<element name="CON-AB" library="SPCoast" package="RJ45-NO-SHIELD" value="">
<attribute name="OPL" value="none"/>
<attribute name="AMP" value="520151-4"/>
</element>
<element name="CON-BA" library="SPCoast" package="RJ45-NO-SHIELD" value="">
<attribute name="OPL" value="none"/>
<attribute name="AMP" value="520151-4"/>
</element>
<element name="CON-BB" library="SPCoast" package="RJ45-NO-SHIELD" value="">
<attribute name="OPL" value="none"/>
<attribute name="AMP" value="520151-4"/>
</element>
<element name="CON1" library="SPCoast" package="RJ24-INVERTED-PINS" value=""/>
<element name="CON2" library="SPCoast" package="RJ24-INVERTED-PINS" value=""/>
<element name="FIDLR" library="SPCoast" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="FIDUL" library="SPCoast" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="LED1" library="SPCoast" package="0603-LED" value="Y"/>
<element name="LEDAA" library="SPCoast" package="0603-LED" value="Y"/>
<element name="LEDAB" library="SPCoast" package="0603-LED" value="Y"/>
<element name="LEDBA" library="SPCoast" package="0603-LED" value="Y"/>
<element name="LEDBB" library="SPCoast" package="0603-LED" value="Y"/>
<element name="R1" library="SPCoast" package="0603-RES" value="2K2"/>
<element name="R2" library="SPCoast" package="0603-RES" value="2K2"/>
<element name="R3" library="SPCoast" package="0603-RES" value="2K2"/>
<element name="R4" library="SPCoast" package="0603-RES" value="2K2"/>
<element name="R5" library="SPCoast" package="0603-RES" value="2K2"/>
<element name="U1" library="SPCoast" package="MAX4702EUE+" value="MAX4702EUE+"/>
<element name="U2" library="SPCoast" package="SOT363" value="74LVC1G97GW"/>
<element name="U3" library="SPCoast" package="SOT363" value="74LVC1G97GW"/>
<element name="U4" library="SPCoast" package="SOT363" value="74LVC1G97GW"/>
<element name="U5" library="SPCoast" package="SOT363" value="74LVC1G97GW"/>
<element name="U6" library="SPCoast" package="SOT363" value="74LVC1G97GW"/>
<element name="U7" library="SPCoast" package="SOT363" value="74LVC1G97GW"/>
<element name="U8" library="SPCoast" package="SOT363" value="74LVC1G97GW"/>
<element name="UA" library="SPCoast" package="MAX4702EUE+" value="MAX4702EUE+"/>
<element name="UB" library="SPCoast" package="MAX4702EUE+" value="MAX4702EUE+"/>
</elements>
<signals>
<signal name="1">
<contactref element="CON1" pad="1"/>
<contactref element="CON1" pad="1@1"/>
</signal>
<signal name="COM1">
<contactref element="U1" pad="2"/>
<contactref element="CON1" pad="2"/>
<contactref element="CON1" pad="2@1"/>
</signal>
<signal name="COM2">
<contactref element="U1" pad="6"/>
<contactref element="CON1" pad="3"/>
<contactref element="CON1" pad="3@1"/>
</signal>
<signal name="COM3">
<contactref element="U1" pad="10"/>
<contactref element="CON1" pad="4"/>
<contactref element="CON1" pad="4@1"/>
</signal>
<signal name="COM4">
<contactref element="U1" pad="14"/>
<contactref element="CON1" pad="5"/>
<contactref element="CON1" pad="5@1"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="12"/>
<contactref element="U1" pad="16"/>
<contactref element="UA" pad="12"/>
<contactref element="UA" pad="16"/>
<contactref element="UB" pad="12"/>
<contactref element="UB" pad="16"/>
<contactref element="CON-AA" pad="1"/>
<contactref element="CON-AB" pad="1"/>
<contactref element="CON-BA" pad="1"/>
<contactref element="CON-BB" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="U8" pad="5"/>
<contactref element="U5" pad="5"/>
<contactref element="U2" pad="5"/>
<contactref element="U6" pad="5"/>
<contactref element="U7" pad="5"/>
<contactref element="U3" pad="5"/>
<contactref element="U4" pad="5"/>
<contactref element="U5" pad="1"/>
<contactref element="U6" pad="1"/>
<contactref element="U7" pad="1"/>
<contactref element="CON2" pad="1"/>
<contactref element="CON2" pad="1@1"/>
</signal>
<signal name="GND">
<contactref element="CON1" pad="6"/>
<contactref element="CON1" pad="6@1"/>
<contactref element="U1" pad="8"/>
<contactref element="CON2" pad="6"/>
<contactref element="CON2" pad="6@1"/>
<contactref element="UB" pad="8"/>
<contactref element="UA" pad="8"/>
<contactref element="CON-AA" pad="6"/>
<contactref element="CON-AB" pad="6"/>
<contactref element="CON-BA" pad="6"/>
<contactref element="CON-BB" pad="6"/>
<contactref element="U8" pad="2"/>
<contactref element="U5" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="U4" pad="2"/>
<contactref element="U7" pad="2"/>
<contactref element="U8" pad="1"/>
<contactref element="LEDAA" pad="C"/>
<contactref element="U5" pad="3"/>
<contactref element="U6" pad="3"/>
<contactref element="U7" pad="3"/>
<contactref element="U6" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="LEDAB" pad="C"/>
<contactref element="U3" pad="1"/>
<contactref element="LEDBA" pad="C"/>
<contactref element="U4" pad="1"/>
<contactref element="LEDBB" pad="C"/>
</signal>
<signal name="A">
<contactref element="CON2" pad="2"/>
<contactref element="CON2" pad="2@1"/>
<contactref element="U1" pad="4"/>
<contactref element="U8" pad="3"/>
<contactref element="U6" pad="6"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="B">
<contactref element="CON2" pad="3"/>
<contactref element="CON2" pad="3@1"/>
<contactref element="UA" pad="4"/>
<contactref element="U8" pad="6"/>
<contactref element="U5" pad="6"/>
</signal>
<signal name="C">
<contactref element="CON2" pad="4"/>
<contactref element="CON2" pad="4@1"/>
<contactref element="UB" pad="4"/>
<contactref element="U7" pad="6"/>
<contactref element="U3" pad="6"/>
</signal>
<signal name="A1">
<contactref element="U1" pad="1"/>
<contactref element="UA" pad="2"/>
</signal>
<signal name="A2">
<contactref element="U1" pad="5"/>
<contactref element="UA" pad="6"/>
</signal>
<signal name="A3">
<contactref element="U1" pad="9"/>
<contactref element="UA" pad="10"/>
</signal>
<signal name="A4">
<contactref element="U1" pad="13"/>
<contactref element="UA" pad="14"/>
</signal>
<signal name="B1">
<contactref element="UB" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="B2">
<contactref element="UB" pad="6"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="B3">
<contactref element="UB" pad="10"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="B4">
<contactref element="UB" pad="14"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="AA1">
<contactref element="UA" pad="1"/>
<contactref element="CON-AA" pad="2"/>
</signal>
<signal name="AA2">
<contactref element="CON-AA" pad="3"/>
<contactref element="UA" pad="5"/>
</signal>
<signal name="AA3">
<contactref element="CON-AA" pad="4"/>
<contactref element="UA" pad="9"/>
</signal>
<signal name="AA4">
<contactref element="CON-AA" pad="5"/>
<contactref element="UA" pad="13"/>
</signal>
<signal name="AB1">
<contactref element="UA" pad="3"/>
<contactref element="CON-AB" pad="2"/>
</signal>
<signal name="AB2">
<contactref element="CON-AB" pad="3"/>
<contactref element="UA" pad="7"/>
</signal>
<signal name="AB3">
<contactref element="CON-AB" pad="4"/>
<contactref element="UA" pad="11"/>
</signal>
<signal name="AB4">
<contactref element="CON-AB" pad="5"/>
<contactref element="UA" pad="15"/>
</signal>
<signal name="BA1">
<contactref element="CON-BA" pad="2"/>
<contactref element="UB" pad="1"/>
</signal>
<signal name="BA2">
<contactref element="CON-BA" pad="3"/>
<contactref element="UB" pad="5"/>
</signal>
<signal name="BA3">
<contactref element="CON-BA" pad="4"/>
<contactref element="UB" pad="9"/>
</signal>
<signal name="BA4">
<contactref element="CON-BA" pad="5"/>
<contactref element="UB" pad="13"/>
</signal>
<signal name="BB1">
<contactref element="CON-BB" pad="2"/>
<contactref element="UB" pad="3"/>
</signal>
<signal name="BB2">
<contactref element="CON-BB" pad="3"/>
<contactref element="UB" pad="7"/>
</signal>
<signal name="BB3">
<contactref element="CON-BB" pad="4"/>
<contactref element="UB" pad="11"/>
</signal>
<signal name="BB4">
<contactref element="CON-BB" pad="5"/>
<contactref element="UB" pad="15"/>
</signal>
<signal name="N$7">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="CON2" pad="5"/>
<contactref element="CON2" pad="5@1"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="N$9">
<contactref element="LEDAA" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="LEDAB" pad="A"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="LEDBA" pad="A"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="LEDBB" pad="A"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="U8" pad="4"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="!B">
<contactref element="U5" pad="4"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="!C">
<contactref element="U7" pad="4"/>
<contactref element="U4" pad="6"/>
</signal>
<signal name="!A">
<contactref element="U6" pad="4"/>
<contactref element="U3" pad="3"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="N$25">
<contactref element="U2" pad="4"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="U3" pad="4"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="U4" pad="4"/>
<contactref element="R5" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
